{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":35,"n_cols":11,"rows_kept":35,"merged":[[0,0,0,10],[1,0,1,10],[31,0,31,10],[32,0,32,10],[33,0,33,10],[34,0,34,10]],"flags":["formulas_cached_only"]}
["    （一）开标一览表"]
["项目名称：2021年8月液压缸采购项目Ⅱ                            项目编号：HGZB21421"]
["序号","资材编号","资材名称","规格型号","技术参数","单位","数量","使用部门","交货时间","含税单价（元）","生产厂家\n（品牌）"]
[1,5722100010,"增压缸","HGZYG40.30L-2.56-00;2440kg","2440kg","台",1,"管加工厂部","2021-11-25"]
[2,7200500035,"液压缸","DYG40X110A-00","额定压力25MPa JB/T 5000","台",2,"管加工厂部","2021-12-10"]
[3,7200100047,"液压缸","CD250E100/70-450A10/02CADMA L10=425","压力等级：25MPa 采用进口密封 连接螺栓12.9级","台",1,"管加工厂部","2021-12-10"]
[4,7200400027,"液压缸","CD250B50/36-340A10/011CADMAC02",null,"台",2,"管加工厂部","2021-12-10"]
[5,7200400025,"液压缸","CD250B50/28-325A10/02CGDMA","06.457-6","台",2,"管加工厂部","2021-12-10"]
[6,7200400077,"液压缸","BG-D-K-F80-478度-Y",null,"台",2,"管加工厂部","2021-12-10"]
[7,7200100375,"脱管机机架锁紧液压缸","按CD250D80/56-130A10/01CADMA标准制造，压力等级250BAR.",null,"台",2,"89热轧","2021-09-26"]
[8,7200100374,"脱管机机架推拉液压缸","按CD250C125/90-2000A10/01CGDMA标准制造，带磁环，不带位移传感器，带耳环，压力等级250BAR",null,"台",1,"89热轧","2021-09-26"]
[9,7200600178,"液压缸","PBICE000;110/95-110","110/95-110；压力25MPa","台",2,"89热轧","2021-12-10"]
[10,7200600176,"液压缸","PBSF30002","63/45-32 活塞加厚","台",4,"89热轧","2021-12-10"]
[11,7501800045,"液压缸活塞杆","H-268-4H-4","45；27.4kg","根",3,"89热轧","2021-09-26"]
[12,7501800046,"液压缸活塞杆","HM28R100","45;24.7Kg","根",2,"89热轧","2021-09-26"]
[13,7200100377,"液压缸","CD250F125/90-380A10/02CADMA","油口G1 1/4；缸径125；杆径90；行程380；耐压等级25MPA;螺栓12.9级","台",2,"180厂部","2021-09-27"]
[14,7200600220,"PG-140平衡油缸","GJ13021","140/70-20","台",2,"89油管车丝委外","2021-10-26"]
[15,7200500012,"料流调节阀液压油缸","100/70-149","带耳环，关节轴承使用国内品牌轴承，密封材质：聚氨酯+丁晴橡胶，工作压力25MPa","台",1,"高炉","2021-12-10"]
[16,7200500015,"炉顶上料闸液压缸","128L-404-6","带耳环，密封材质：尼龙夹布V组，工作压力25MPa","台",1,"高炉","2021-12-10"]
[17,7200500016,"炉顶上下密液压缸","80*56-340","带耳环，密封材质：尼龙夹布V组，工作压力25MPa","台",1,"高炉","2021-12-10"]
[18,7200500013,"炉顶二次均压液压缸","WYX08CD250A63/35-470.02ADMA","带耳环，密封材质：尼龙夹布V组，工作压力25MPa","台",1,"高炉","2021-12-10"]
[19,7000700015,"大包热修位液压站","HGLG090602","油箱300L;系统压力200bar;阀组一用一备;阀块分开;配电控部分;要求操作动作按钮时液压泵启动;松开按钮时液压泵关闭","套",1,"炼钢厂部","2021-09-26"]
[20,7200600011,"摆动液压缸","50/36-740","缸径Φ50,杆径Φ36,行程740 工作环境温度-20℃~140℃ 工作压力20MPa,试验压力25MPa 活塞及活塞杆采用V型组合耐高温密封 韶关液压件厂 工作介质水乙二醇液压油","台",2,"炼钢厂部","2021-12-10"]
[21,7200600055,"热修位液压缸","90/45-203","配进口密封 缸径Φ90,杆径Φ45,行程203 工作环境温度-20℃~140℃ 工作压力20MPa,试验压力25MPa 活塞及活塞杆采用V型组合耐高温密封 工作介质水乙二醇液压油","台",2,"炼钢厂部","2021-12-10"]
[22,7200100152,"液压缸","CDH1MT4/80/56-300A1X/B1CSDMWW+GAS40 XV=342","缸径Φ80,杆径Φ56,行程300 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台",1,"340热轧","2021-12-10"]
[23,5722100033,"预密封缸","FPWV220*270-00;","部件；490kg;工作压力16MPa;审核图纸","台",1,"180厂部","2021-11-26"]
[24,7200200066,"液压缸","Z0745.05.02.04","额定压力25MPa JB/T 5000","台",2,"180厂部","2021-11-10"]
[25,7200500034,"液压缸","CD250B80/56-90A10/02CADMA","额定压力25MPa JB/T 5000","台",2,"180厂部","2021-12-10"]
[26,7200100376,"液压缸","CD350E63/45-650B10/02CADMA L10=200","缸径63；杆径45；行程650；L10＝200；压力等级：25MPa；连接螺栓12.9级","台",5,"180厂部","2021-08-27"]
[27,7200100174,"液压缸","SF600179","额定压力25MPa JB/T 5000","台",4,"180厂部","2021-12-10"]
[28,7200200005,"炉底机械液压缸","HG18002690017DR5004ME003-110","100/70-600,,JB/T 5000","台",1,"180厂部","2021-12-10"]
["注：1、投标报价含税，税率13% ；                                                                                                                          2、生产厂家要求全称填写准确无误 ；                                                                                                                     3、每个单项只允许一个有效报价，须按此表顺序与格式填报，不得打乱报价顺序（未报价的行、列不得删除）；"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":18,"n_cols":4,"rows_kept":18,"merged":[[0,0,0,3],[1,0,1,3],[3,0,5,0],[3,3,5,3],[6,0,13,0],[6,3,13,3],[14,0,14,3],[15,0,15,3],[16,0,16,3],[17,0,17,3]],"flags":["formulas_cached_only"]}
["   （二）商务/技术偏离表"]
["项目名称：2021年8月液压缸采购项目Ⅱ                             项目编号：HGZB21421"]
["偏离类型","序号","招标方要求内容","投标方偏离内容"]
["商务偏离"]
[]
[]
["技术偏离"]
{"$rows_empty":7}
["注：1、如商务无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标方要求内容有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n    2、如技术无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标内容（规格描述、技术要求及标准、交货期等内容）有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]