{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":36,"n_cols":13,"rows_kept":36,"merged":[[0,0,0,12],[1,0,1,12],[32,0,32,12],[33,0,33,9],[34,0,34,9],[35,0,35,9]],"flags":["formulas_cached_only"]}
["（一）开标一览表"]
["项目名称：2022年7月电气备件采购项目Ⅱ                    项目编号：HGCGD22098"]
["序号","资材编号","资材名称","规格描述","技术参数","执行标准","单位","数量","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,6400600441,"凸轮开关","TKE4-0-T/201-B/RMF5","电压10-30V；电流200mA；海光机械电器厂","GB/T 1408.10-1999","台",2,"180厂部","2022-09-10"]
[2,6400300235,"接近开关","NJ1,5-8GM-N-Y18488","开关功能: 常闭 (NC), 输出类型: NAMUR, 安装: 齐平, 输出类型: 2 线, 螺纹模具: M8, 结构类型: 圆柱形，螺纹, 系列: 圆柱形; 防护等级: IP67, 材料: PUR.","GB/T14048.10-2008","只",10,"管加工厂部","2022-09-10"]
[3,6300700061,"操作屏","smart700iev3(含程序及调试)","电压DC24V，RS422/RS485，USB","IEC61508","块",1,"高炉","2022-09-10"]
[4,6000400020,"合闸电磁铁","220VDC 205Ω",null,"GB14048.4-93","只",10,"炼钢厂部","2022-09-10"]
[5,6400400007,"增量编码器","DGS60-G4B04096 德国IEC947","电源电压DC10-30V，脉冲数1024个/圈","德国IEC947","只",1,"炼钢厂部","2022-09-10"]
[6,6300500265,"串口卡","MOXA CP-118U","8口RS-232/422/485多串口卡","IEC61000-4-2","只",2,"炼钢厂部","2022-09-10"]
[7,6100300159,"户内六氟化硫断路器小车","LN2-40.5/1600-25","额定电压40.5KV 额定电流1600A","JB/DQ2553-1989","只",3,"炼钢厂部","2022-09-10"]
[8,6400600196,"压力传感器","5705-BSPX1052 350BAR","精度等级正负0.5% 过载压力1052Bar 测量范围0-350Bar 测量介质温度-25℃ - +80℃ 模拟输出 4-20毫安 耐振≤10g/0..500HZ 耐冲击≤50g/11ms","DIN16086-2006","只",5,"180厂部","2022-09-10"]
[9,6700100045,"数字式厂用变保护测控装置","PDS-765 工作电源DC220V 遥信变位响应时间＜1 s",null,"GB/T21705—2008","只",1,"炼钢厂部","2022-09-10"]
[10,6100100080,"数字式电动机保护测控装置","PDS-766 整组动作时间(包括出口继电器动作时间)电流速断保护：≤35ms 带时限保护动作时间与整定值的误差:?≤+20ms",null,"GB/T21705-2008","台",1,"炼钢厂部","2022-09-10"]
[11,6100100088,"数字式线路保护测控装置","PDS-761 DC220V允许偏差：－20％～＋15％ 5A 测量误差：不大于 0.02 （ 相 对 误 差 ）",null,"GB/T25840-2010","台",1,"炼钢厂部","2022-09-10"]
[12,6100100150,"控制变压器","BK-50","380V/36V;50VA",null,"只",5,"高炉","2022-09-10"]
[13,7502500028,"轴流风机","150FZY2-S","65W","GB/T13933-2008","台",5,"219厂部","2022-09-10"]
[14,6600400210,"配电器","DGP-1100;4-20mA","DC24V",null,"台",4,"219厂部","2022-09-10"]
[15,6400400115,"绝对值编码器网络插头","TMSP12FD-M4","12  米","GB/T20281-2006","根",5,"89油管车丝委外","2022-09-10"]
[16,6000300235,"瓦格拉锯电机风轮","YF-1","直径：250mm,高：64mm, 孔：19mm,键槽：6mm","GB/T 1236-2000","个",5,"89油管车丝委外","2022-09-10"]
[17,6000300236,"瓦格拉锯电机风轮","YF-2","直径：180mm,高：80mm, 孔：19mm,键槽：6mm","GB/T 1236-2000","个",5,"89油管车丝委外","2022-09-10"]
[18,5300100969,"天车超重限载器套件","QCX-M-5t+5t（带双传感器及8寸大屏显示器）","带2个5t传感器及8寸显示屏；","GB14048","套",2,"89油管车丝委外","2022-09-26"]
[19,6300600078,"喷码机主控板","PMC-PJ1A","IC4-2216-J主控板","IEC61509","块",1,"89油管车丝委外","2022-09-10"]
[20,6100900049,"不锈钢电阻器","RS54-280M-8/5H","75KW","IEC61508","套",1,"炼钢厂部","2022-09-10"]
[21,6300400011,"PLC 电源模块","1756-PA72","AB","GBT15969","块",2,"管加工厂部","2022-09-10"]
[22,6600400253,"前置器","1142-DR-5850","NCPU, Driver, 5&8mm, 5m system  AB","JB/T11279-2012","个",3,"高炉","2022-09-10"]
[23,6200100035,"直流调速装置","DCM-CON70-V 0","四相限控制 带profibus-dp通讯板 小装置控制大功率晶闸管整流装置 带励磁控制单元220V,39A 晶闸管主回路直流输出电压DC850V 额定输出直流电流3162A，直流电机带编码器速度反馈，可弱磁升速。",null,"套",1,"219厂部","2022-09-10"]
[24,6100300155,"断路器:","DZ158-100A/3P","380V 3P 100A","JB/T8735.2011","只",10,"180厂部","2022-09-10"]
[25,6300500256,"位移监测模块","EK-C6682","EK-C6682双通道位置监测模块，可接收两个标准的电涡流传感器输入信号，监测轴端止推轴承的轴向位置，电源：220VAC",null,"个",1,"高炉","2022-09-10"]
[26,6400200047,"光电开关","WL45-P260","矩型 金属 直接反射型 供电电压10~60VDC PNP型 常开点/常闭点 接线端子 IP67","EN 60947-5-2:2007","只",5,"180厂部","2022-08-10"]
[27,6400200029,"反光镜","OP61",null,"GB/T23110-2014","套",19,"180厂部","2022-08-10"]
[28,6400400116,"编码器","AFM60A-S4NB018X12","SICK  输入24V 绝对值","IEC61800","套",1,"180厂部","2022-08-10"]
[29,6400200052,"光电开关","WT45-P260 1009108","矩型 金属 直接反射型 供电电压10~30VDC 50mm PNP型 常开点/常闭点 80Hz 接线端子 IP67","GB/T23110-2014","块",18,"180厂部","2022-08-10"]
["注：1、投标报价含税，税率13%                      2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2022年7月电气备件采购项目Ⅱ        项目编号：HGCGD22098"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":4,"n_cols":1,"rows_kept":4,"merged":[[0,0,0,8],[1,0,1,8],[2,0,2,8],[3,0,3,8]],"flags":["formulas_cached_only"]}
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]