{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":81,"n_cols":12,"rows_kept":81,"merged":[[0,0,0,11],[1,0,1,11],[77,0,77,8],[78,0,78,8],[79,0,79,8],[80,0,80,8]],"flags":["formulas_cached_only"]}
["（一）开标一览表"]
["项目名称：2023年5月电气备件采购项目                   项目编号：HGJY-G2023060"]
["序号","资材编号","资材名称","规格描述","技术参数","执行标准","单位","数量","申请部门","交货期","含税单价（元）","生产厂家"]
[1,6100500353,"时间继电器","SK4-220d；0.1～3S","通电延时型空气延时头；延时动作时间0.1～3S；触头额定电流：0.95A主触头触点形式：双断电；工作条件：周围空气温度-50℃—+40℃，24小时的平均值不超过+35℃；空气的相对湿度为不超过50%；安装地点海拔不超过2000M；","GB14048.4-2010","只",20,"340热轧","2023-06-30"]
[2,6400400049,"增量编码器","DKS40-E5J01000 带弹性联轴器9402 8*8 SICK","增量型 金属外壳 脉冲数1024 侧向电缆直接 10 V ... 30 V 供电，符合标准DIN EN 61000-6-4，DIN EN 61000-6-2","EN61000-6-2","只",2,"720厂部","2023-06-30"]
[3,6100300074,"断路器","DZ47-60,2P 20A","Ue:690V.50/60Hz","GB14048.2-2001","只",20,"340热轧","2023-06-30"]
[4,6100600263,"快速熔断器","NGTC00","800V/125A",null,"只",12,"180厂部","2023-06-30"]
[5,6400200013,"对射式光电开关","OM30-EVP6 ELCO JT 2-30s/1499","外形:圆柱型 外壳材质:金属 检测模式/感应类型:对射式（接收器） 供电范围:10-30VDC 感应范围:0-25m 输出形式:PNP 输出特性:常开1点，常闭1点 接线方式:导线输出连接 防护等级:IP67","JT 2-30s/1499","只",16,"管加工厂部","2023-06-30"]
[6,4100400156,"铜接线鼻子","C240-16",null,null,"只",50,"炼钢厂部","2023-06-30"]
[7,6100600084,"熔断器","RS96B-300A/500V","圆管螺栓连接式半导体快速熔断体 额定电压500V 额定电流300A","GB13539.1","只",50,"炼钢厂部","2023-06-30"]
[8,6100600085,"熔断器","RS96B-400A/500V","圆管螺栓连接式半导体快速熔断体 额定电压500V 额定电流400A","GB13539.1","只",20,"炼钢厂部","2023-06-30"]
[9,6400300206,"行程开关","LX33-32","触头AC500V;两对触头(常开常闭各一对);容量10A带重锤","JB/T 5553-2006","个",15,"炼铁厂部","2023-06-30"]
[10,6100500373,"中间继电器","46.52.9.024.0040","8针;24VDC;8A;250V~;finder",null,"只",60,"720厂部","2023-06-30"]
[11,4100400175,"端子排短接片","280-402  25PCS","WACO","IEC947-7-1","片",300,"340热轧","2023-06-30"]
[12,6300600048,"比例阀电源板","VT-VSPA2-50-10/T5",null,"GB/T14048.10-2008","块",2,"340热轧","2023-06-30"]
[13,4100500381,"按钮","LA42P-11/GS","TAYEE 1NC;10A 600V AC;1A 250V DC;Uimp=6KV Ui=500V;TIGHTENING TOROUE 1.2Nm","GB14048.5  GB/T14048.1","只",20,"340热轧","2023-06-30"]
[14,4100500382,"按钮","LA42P-11/RS","TAYEE 1NC;10A 600V AC;1A 250V DC;Uimp=6KV Ui=500V;TIGHTENING TOROUE 1.2Nm","GB14048.5  GB/T14048.1","只",20,"340热轧","2023-06-30"]
[15,4100500004,"按钮","C0B 63A AC250V5A","AC500V.2A","JB/T 570-1998","只",10,"340热轧","2023-06-30"]
[16,6400600185,"限位开关","XCK-J10513","240V 3A 一常开一常闭 防护等级IP66 标准:IEC60947-5-1 GB14048.5","GB/T2951.11-2008","只",10,"720厂部","2023-06-30"]
[17,4100400054,"电缆中间接头铜连接管","*","T2紫铜 70mm2","JB/T7435","只",20,"炼钢厂部","2023-06-30"]
[18,4100400055,"电缆中间接头铜连接管","*","T2紫铜 95mm2","JB/T7435","只",20,"炼钢厂部","2023-06-30"]
[19,4100400056,"电缆中间接头铜连接管","*","T2紫铜 150mm2","JB/T7435","只",20,"炼钢厂部","2023-06-30"]
[20,4100400057,"电缆中间接头铜连接管","*","T2紫铜 185mm2","JB/T7435","只",20,"炼钢厂部","2023-06-30"]
[21,4100400058,"电缆中间接头铜连接管","*","T2紫铜 120mm2","JB/T7435","只",20,"炼钢厂部","2023-06-30"]
[22,4100400059,"电缆中间接头铜连接管","*","T2紫铜 50mm2","JB/T7435","只",20,"炼钢厂部","2023-06-30"]
[23,4000400009,"电热吹风","MODEL CS-2000","电压220V-240V 2000W 热度:100-650度 冷/热风","KS C9311-2002","台",1,"炼钢厂部","2023-06-30"]
[24,4000200001,"10KV母线热缩套","*","铜排规格60*6","GB/T 14823.4-1993","米",30,"炼钢厂部","2023-06-30"]
[25,4000200002,"10KV母线热缩套","*","铜排规格80*6","GB/T 14823.4-1993","米",30,"炼钢厂部","2023-06-30"]
[26,6300500068,"光纤","光纤 LWL Formkabel lsatz FSH",null,null,"根",3,"180厂部","2023-06-30"]
[27,6000200465,"真空断路器","3AH4305-4 Ur=36KV/Isc=31.5KA/Ir=2000A/屏柜NX-40.5 带小车 德国IEC947","德国IEC947","德国IEC947","台",1,"炼钢厂部","2023-06-30"]
[28,6400500902,"枪内专用线","ADE-LDRX-QNX","配测温探头，长度：1.6m",null,"套",1,"炼铁厂部","2023-06-30"]
[29,6400500903,"枪外专用线","ADE-LDRX-QWX","长度：25m，12芯+视频线",null,"套",1,"炼铁厂部","2023-06-30"]
[30,6100600106,"快熔","NGTC2  1000V/400A",null,"GB/T13539 IEC 60270","个",12,"180热轧","2023-06-30"]
[31,4100400065,"堵油型铜接线鼻子","*","25mm2","GB/T 14315-2008","只",50,"720厂部","2023-06-30"]
[32,4100400181,"端子排","JX2-60A","500V",null,"条",15,"能源厂部","2023-06-30"]
[33,4100400023,"PVC电缆号码套管","*","φ4.0 100m/卷 塑料 阻燃性VW-1 耐温200℃ 内径4mm2","GB/T 28605-201","卷",1,"能源厂部","2023-06-30"]
[34,4100400024,"PVC电缆号码套管","*","φ2.5 100m/卷 塑料 阻燃性VW-1 耐温 200℃内径2.5mm2","YD/T841.2-2008","卷",1,"能源厂部","2023-06-30"]
[35,4100300047,"内制编码器拉绳开关","JX-LS-DZ","电压：AC220V,通讯方式：CAN，硬接点数量：2常开2常闭，触点容量：DC24/15A-380/10A,复位方式：手动复位，编码设置：0-254，设置方式：红外遥控，显示方式：跳动提示，材质：铝压铸","JB/T  10960-2010","个",16,"炼铁厂部","2023-06-30"]
[36,4000400051,"万能转换开关","LW39-16","Ui660V Ith16A 3档","GB 2682-81","只",20,"炼铁厂部","2023-06-30"]
[37,6600200863,"取温取压探头组件","FPI6.151.194","探杆长度1700mm;材质不锈钢;带涂层","HJ76-2017","套",1,"炼铁厂部","2023-06-30"]
[38,6600200864,"电加热探杆","35*1700","探杆长度1700mm;材质不锈钢;220V-400W","HJ76-2017","只",1,"炼铁厂部","2023-06-30"]
[39,6600200865,"加热盒气体室","FPI5.814.476","CEMS-2000.  V4.0用;光程800mm","HJ76-2017","台",1,"炼铁厂部","2023-06-30"]
[40,4000200359,"35KV穿墙套管","CWC-35/2000A","35KV/2000A;尺寸：L:950\\L1：790\\L2：422\\L3：12\\d1:16\\d2:45\\a:200","JB/DQ2553-1989","只",9,"炼钢厂部","2023-06-30"]
[41,6300700072,"综合显示大屏","BCD4P-AN2P-176","VOITAGE:100-240VAC/50-60HZ","Q/IBRF7-2013","台",1,"炼钢厂部","2023-06-30"]
[42,7001900016,"油漆喷印机 自闭快插","H-16PL01",null,"GB/T1723-1993","只",4,"180热轧","2023-06-30"]
[43,6100700025,"电流互感器","CP62/20.80/0.1A","CLASS:1.0  2.5VA; 50/60HZ; 0.72/3KW",null,"只",2,"180热轧","2023-06-30"]
[44,6200200204,"变频器","20G11NC043JA0NNNNN 22Kw PowerFIex755 E0.967X","进线电压：3相 380V-480VAC 额定功率22KW 重载功率18.5KW 额定电流43A","E0.967X","台",4,"720厂部","2023-07-13"]
[45,6200100091,"变频器","MD480T11GB","11KW","EN61800-3","台",15,"720厂部","2023-06-30"]
[46,6300500229,"网卡","20-750-ENETR","PowerFlex 753系列变频器以太网卡","德国IEC947","个",4,"720厂部","2023-06-30"]
[47,6400400055,"绝对编码器","RSP02-58-13+12-3-B-W1-DS","Profibus-Dp总线型绝对值型多圈编码器 主体尺寸:φ58 安装方式:φ36夹紧法兰，轴长20MM 10-30VDC供电 圈数:4096/单圈位置数:8192","IEC60947-5-1","只",3,"720厂部","2023-07-13"]
[48,6300700071,"触摸屏","MT8102iE","10.1寸显示屏;分辨率1024*600;防护等级IP65;带下载线","GBT 2828","块",1,"炼钢厂部","2023-06-30"]
[49,4100400288,"电缆护层保护器","LHQ-35","额定电压35KV;工频耐受/时间(5/4)KV/S; 10KA雷电冲击电流下残压≤12KVP;直流参考电压≥5.5KV;2ms方波通流容量400A;0.75U1mA下的泄漏电流≤50UA","DL/T401-2002","个",10,"炼钢厂部","2023-06-30"]
[50,6300300134,"多通道高速激光通讯模块","ZYT-CP134U","电源+5V;PCI串口通讯;提供4个RS-422/485串口;速率50bsp-921.6kbps;工作温度0-55度","IGB/T 176-2017","块",1,"炼钢厂部","2023-06-30"]
[51,4100400290,"集电器","PB39-DC-I-1200A","容量1200A","JT/T806.3-2011","个",10,"炼钢厂部","2023-06-30"]
[52,6400300241,"起升高度限制器","QGX-DE-2A","速比1:50;触头容量2A","JB/T5553-2006","台",5,"炼钢厂部","2023-06-30"]
[53,6100900142,"现场动力柜","800*600*1800mm(宽*深*高），不锈钢","熔断器式隔离开关，WGR-320/3P，含300A熔芯1个；塑壳断路器 NSX250N TMD 250A 1个，内可控制污泥电机1.5KW  搅拌电机1.5KW*8台的控制回路；检修电源开关 NSX100N TMD 100A 2个；天车电源750W NSX100N TMD 63A 开关2个；",null,"个",1,"340热轧","2023-06-30"]
[54,6100900143,"分线箱","400*500*300mm，冷板,内装铜排等","支架 镀锌角钢L50*50*5；槽钢底座  10#镀锌槽钢；铜鼻子、金属软管；电缆头；铜排40*4 9台 40*3 6台 30*4 4台 25*3 3台 20*3 3台","JB/T8219-1999","个",15,"340热轧","2023-06-30"]
[55,6100400401,"中间继电器","SZR-LY4-N1-DC24","线圈电压24VDC  额定接触电流 10A","GB/T 36640-2018","个",2,"能源厂部","2023-06-27"]
[56,6100400400,"固态继电器","WYG1C20Z4","MAS 240VAC 20A","GB/T 36640-2018","个",2,"能源厂部","2023-06-27"]
[57,6200200892,"变频器","PowerFlex 753；20F11FC060JA0NNNNN  AB","输入电压：400V交流 输入频率：三相，47-63HZ：输出电压：0-400V 输出电流：60A 输出频率：三相，0-400HZ 一般负载：30KW","IEC61800","台",2,"炼铁厂部","2023-06-27"]
[58,6400600522,"压力传感器","ISE30A-01-D","SUP 12-24VDC  CLASS2 40mA MAX\n\nOP.PRESS -0.1-1.0MPa","GB/T15478-1995","只",4,"180热轧","2023-06-30"]
[59,6100100223,"开关柜智能操控装置","DN8310/HS2/X/DC220V/Z/S","装置电压DC220V 温控电压AC220V 温湿控制2路  开关旋钮1个  带电显示","IEC255-22","台",1,"能源厂部","2023-06-27"]
[60,5300300802,"浮球液位控制器","UHK30-500-5m","UHK30-500-5m  原厂家：上海天敏","JB/T2785-2010","件",2,"720厂部","2023-07-27"]
[61,6300100126,"CPU模块","AS228T-A","带16点DI,12点DO,64k容量,内建以太网口,RS485*2,集成CANOPEN,带CANOPEN电缆(UC-CMC003-01A)","IEC60130","台",1,"720厂部","2023-06-30"]
[62,6300400094,"电源模块","AS-PS02","输入100-220VAC,输出24VDC(2A),PLC机架电源","IEC60130","台",1,"720厂部","2023-06-30"]
[63,6200200891,"伺服驱动器","ASD-A3-1B43-M","11KW,输入400vac,A3系列,CANOPEN通讯","IEC60130","台",1,"720厂部","2023-06-30"]
[64,4100800114,"凸轮控制器","TKD6-3002C/300A","电压:DC10-30V,电流:200MA","GB/T1408.10-1999","台",1,"89油管车丝委外","2023-06-30"]
[65,5300300866,"GF1C机车电瓶箱门装配总成","GK1C机车：长420mm，宽1100mm",null,null,"条",4,"物流中心","2023-06-30"]
[66,6400200105,"激光测距控制器","HD-9020","U:220V/AC  I:5A,检测距离0-20m","JB/T6475-1992","台",2,"89油管车丝委外","2023-06-30"]
[67,4000200364,"工业插头","KMS-025 32A-6h","三相五极，电流32A,电压220-380VAC/240-415VAC,3P+N+E,IP44,","IEC309-2","只",100,"89油管车丝委外","2023-06-30"]
[68,4000200365,"工业插座","KMS-325 32A-6h","三相五极暗装直插，电流32A,电压220-380VAC/240-415VAC,3P+N+E,IP44,","IEC309-2","只",100,"89油管车丝委外","2023-06-30"]
[69,6200300097,"中频控制电路板","DLJ-6  1-2.5KHz","输入电源交流17V ，输出频率1000-2500HZ","SJ/T10616-1995","块",2,"89油管车丝委外","2023-06-30"]
[70,6500200138,"散热风机","艾默生UL33-0400L UPS散热风机型号W2S130-AA03-01","230V、45W",null,"个",1,"持续改进部","2023-06-30"]
[71,6100100060,"控制变压器","BK-150","220V/380V/12V/24V/36V 150VA GB 1094.11-2007","GB 1094.11-2007","台",3,"219厂部","2023-06-30"]
[72,4200700015,"电源适配器","DJ-U48S-12IN","AC220V OUT:12VDC-4A DAJING","GB4943.1-2013","台",10,"89油管车丝委外","2023-06-30"]
[73,6400400018,"绝对编码器","CE65M Nr:110-02904 Sn0621 11-27vDC pruif Nr.30253 6404 TR公司 D-78647","Schritte/Umdrehung Prog.(Max:4096) Umdrehung Prog.(Max:4096) Schnittstelle/Code SSI/Prog:Stebel.Nersion 2293 AN00 Ausgangspege1 RS422 option Trwinprong:Spannung:11-27vDC pruif Nr.30253 06404 绝对值型 金属外壳 外形尺寸∮65mm SSI输出 符合标准DIN EN 61000-6-4，DIN EN 61000-6-2",null,"只",2,"219厂部","2023-06-30"]
[74,6100600268,"熔断器","PC27UD31C15CP50","3100VAC;1500A;Ferraz Shawmut",null,"个",3,"720厂部","2023-06-30"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2023年5月电气备件采购项目        项目编号：HGJY-G2023060"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}