{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["一、开标一览表","二、商务 技术偏离"],"read":"whole","date_system":"1900"}

{"sheet":"一、开标一览表","index":0,"n_rows":23,"n_cols":11,"rows_kept":23,"merged":[[0,0,0,10],[1,0,1,5],[1,6,1,10],[19,0,19,10],[20,0,20,10],[21,0,21,10],[22,0,22,3]]}
["开  标  一  览  表"]
["项目名称：2023年6月-2024年5月仪器仪表年标采购项目                            项目编号：HGJY-G2023069"]
["序号","物料编码","物料描述","规格描述","技术参数","单位","数量","交货日期","含税单价（元）","生产厂家","备注"]
[1,4201700010,"对讲机","LT-3268 TIA/EIA-603","TIA/EIA-603","台",700,"以订单为准",null,null,"需求量以订单为准"]
[2,6500400149,"工业电视网络960P红外枪式摄像机","BL-CE5720B-096B","含支架及2A室外防水电源","台",140,"以订单为准",null,null,"需求量以订单为准"]
[3,6400500127,"探伤机 漏磁纵向探头架","6.085-795-02 MIL-STD-1344A","附合格证 附性能测试报告","件",9,"以订单为准",null,null,"需求量以订单为准"]
[4,6400500234,"超声波探伤仪","HS600","HS600附合格证 附性能测试报告","台",4,"以订单为准",null,null,"需求量以订单为准"]
[5,6400600109,"红外测温仪","ST300-AHH","700-1400℃ 双色 精度1% 发射率:0.3～1.0数字可调 24VDC供电 4~20mA输出 带显示表及70米电缆 带安装附件","台",5,"以订单为准",null,null,"需求量以订单为准"]
[6,6500400082,"工业电视 网络硬盘录像机","BL-P1604-A","提供免费集中监控软件，以太网接口LAN和IPC接口，16通道以上连接高清数字摄像机","台",34,"以订单为准",null,null,"需求量以订单为准"]
[7,4200800012,"对讲机","GM360","配220V转换器","台",28,"以订单为准",null,null,"需求量以订单为准"]
[8,6600200679,"数字式高精度称重传感器","SLC820-50t","1、制造商: 梅特勒-托利（常州）精密仪器有限公司；2、结构:压式柱型,DWP,不锈钢材材料外壳，焊接密封；3、额定容量: 50T；4、蠕变(30分钟):±0.013%F.S；5、非线性:±0.010%F.S；6、滞后:±0.016%F.S；7、重复性：±0.005%F.S；8、防雷击能力（最大测试指标）： 80000A；9、IP防护等级： IP68/IP69K；10、使用温度范围 -40C~+55C；11、最大安全过载: 200%F.S","个",4,"以订单为准",null,null,"需求量以订单为准"]
[9,6400600181,"无线测温枪","KZ-888CQN-604-SH","整长4.5米 前节1.2米 配线测温枪机芯 S分度号，测温范围：600-1769℃ 通信范围70m","把",12,"以订单为准",null,null,"需求量以订单为准"]
[10,6400600110,"红外测温仪","MTX50HL","0-700℃ 单色 精度1% 带安装附件","台",7,"以订单为准",null,null,"需求量以订单为准"]
[11,6500200124,"手持终端扫码器","UROVO DTSOQ","操作系统  Android 9.0；RAM：4GB ROM：64GB；5.7英寸彩色全面屏（1080×2160）；触摸屏  支持多点触控、手套触摸，带水操作和被动笔签名，康宁玻璃盖板；3.85V 4300mAh 可充电锂电池；（多功能单座充，充（5主机），扫描手柄，RFID手柄，身份证模块，大电池，光学指纹模块，腕带，保护膜，背包，胶套，双色保护套）","台",20,"以订单为准",null,null,"需求量以订单为准"]
[12,6600400205,"激光光幕检测仪","JNAHG-172-8-108","DC24V,检测距离0.3～8米;光轴间距35毫米","台",6,"以订单为准",null,null,"需求量以订单为准"]
[13,4000500058,"电缆桥架盖板","2000mm*600mm*1.5mm（长*宽*厚）","材质：镀锌钢板","米",750,"以订单为准",null,null,"需求量以订单为准"]
[14,6600200068,"三相三线电子式多功能电能表","DSSD331","3*100V/3*1.5(6)A/50Hz 0.5级","块",29,"以订单为准",null,null,"需求量以订单为准"]
[15,4100500053,"耐高温铠装线","NRRGF-WB8C6S-4",0,"只",50,"以订单为准",null,null,"需求量以订单为准"]
[16,6600200107,"超声波测厚仪","CTS-30A","附合格证","台",17,"以订单为准",null,null,"需求量以订单为准"]
["注：1、投标报价含税，税率13%                                                                                     \n2、生产厂家要求全称填写准确无误"]
["投标人：（盖单位章）"]
["法定代表人或其委托代理人：（签字或盖章）"]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离","index":1,"n_rows":18,"n_cols":4,"rows_kept":18,"merged":[[0,0,0,3],[1,0,1,3],[3,0,5,0],[3,3,5,3],[6,0,13,0],[6,3,13,3],[14,0,14,3],[15,0,15,3],[16,0,16,3],[17,0,17,3]]}
["   （二）商务/技术偏离表"]
["项目名称：2023年6月-2024年5月仪器仪表年标采购项目  \n项目编号：HGJY-G2023069"]
["偏离类型","序号","招标方要求内容","投标方偏离内容"]
["商务偏离"]
[]
[]
["技术偏离"]
{"$rows_empty":7}
["注：1、如商务无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标方要求内容有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n    2、如技术无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标内容（规格描述、技术要求及标准、交货期等内容）有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n"]
["投标人：                         （盖单位公章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]