{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":50,"n_cols":12,"rows_kept":50,"merged":[[0,0,0,11],[1,0,1,11],[46,0,46,8],[47,0,47,8],[48,0,48,8],[49,0,49,8]],"flags":["formulas_cached_only"]}
["（一）开标一览表"]
["项目名称：2024年5月电气备件采购项目                    项目编号：HG JY-G2024055"]
["序号","资材编号","资材名称","规格描述","技术参数","执行标准","单位","数量","申请部门","交货期","含税单价（元）","生产厂家"]
[1,6100500430,"大功率继电器","JQX-38F 3Z","线圈电压24VDC;辅助触点负载40A;辅助触点三开三闭","GB/T14048","只",20,"炼钢厂部","2024-07-27"]
[2,4100500156,"断路器","DZ10-250","100A",null,"只",5,"720厂部","2024-07-27"]
[3,6100300065,"断路器","DZ10-250/320；150A","150A","GB/T14048","只",3,"720厂部","2024-07-27"]
[4,4100400176,"端子排卡子","249-116",null,"IEC947-7-1","个",100,"219厂部","2024-07-27"]
[5,6400600022,"安全开关","LX8-5",null,"GB/T5465.2-1996","只",10,"物流中心","2024-07-27"]
[6,4100800125,"联动台手柄","YGK3 两方向联动台手柄","中位不通，前进和后退2档，前一 1通，前二1 2通，后退一样","GB14048-200","个",6,"物流中心","2024-07-27"]
[7,6100300332,"空气开关","CDP6-32","CKD6E机车用，32A","GB/17701-2008","件",15,"物流中心","2024-07-27"]
[8,6100300333,"自动脱扣开关","DZ5B-50，GK1C机车（0324）","380V，40A","GB/17701-2008","只",5,"物流中心","2024-07-27"]
[9,6100300334,"自动脱扣开关","GK1C机车（0262）DZ5B-50","380V，30A","GB/17701-2008","只",5,"物流中心","2024-07-27"]
[10,6400600611,"位移传感器","EHM0230MEH21A01含磁环OD33 201542-2","公制螺纹M18x1.5/外管直径10mm, 标称测量长度230mm,4-20mA输出信号,5m PUR电缆,","GB/T28857-2012","只",3,"89热轧","2024-07-27"]
[11,4300600063,"开口PP阻燃穿线波纹管","内径Φ12mm","阻燃防水，防踩变形","JB/T10358-2002","米",400,"89管加工热处理","2024-07-27"]
[12,4300600064,"开口PP阻燃穿线波纹管","内径Φ22mm","阻燃防水，防踩变形","JB/T10358-2002","米",400,"89管加工热处理","2024-07-27"]
[13,6100400055,"接触器","CJX8-105","140A 690V 线圈电压220V","GB/T19582-2008","只",4,"炼钢厂部","2024-07-27"]
[14,4000200041,"分流器","FL-2/75A/75mV","75A/75mV","GB/T16894","只",2,"能源厂部","2024-07-27"]
[15,6400300242,"振动传感器","CST51301-G03","4-20mA  7.87mV/μm   DC12V-35V  0-125μm","GB/T14048","个",1,"能源厂部","2024-07-27"]
[16,6400600593,"MTS磁致伸缩位移传感器","RH5MA0050M01D701S1011G1","电源电压24VDC;输出类型SSI;数据长度25bit;数据格式;格雷码;分辨率5μm;标准行程50mm;连接类型;M16公接头（7针）;正向测量;异步模式;配201542-2磁环","JB/T10726-2007","台",2,"炼钢厂部","2024-07-27"]
[17,6400400007,"增量编码器","DGS60-G4B04096 德国IEC947","电源电压DC10-30V，脉冲数1024个/圈","德国IEC947","只",2,"炼钢厂部","2024-07-27"]
[18,6400100049,"火焰信号探测器","BC1000A0220U/E","电源：220VAC;50/60Hz;8W","GB15631-1995","台",1,"炼钢厂部","2024-07-27"]
[19,6400600606,"磁簧式传感器","CMSE-020","两线制;使用电压5-240VAC/DC;防护等级IP64","GB/T 23110-2008","个",10,"炼钢厂部","2024-07-27"]
[20,6300700086,"嵌入式一体化触摸屏","TPC1031Ki","电源24VDC;功耗≤30W;环境0-50℃","GB4943.1","块",1,"炼钢厂部","2024-07-27"]
[21,6300700085,"嵌入式一体化触摸屏","TPC7022Hj","输入;24V DC/300mA MaX;环境;0℃-50℃","GB4943.1","块",1,"炼钢厂部","2024-07-27"]
[22,6100100250,"充电模块","SD-230/10","交流输入380VAC 50HZ;直流输出220VDC 10A;电压变化范围AC323-437V","DL/781-2001","块",3,"炼钢厂部","2024-07-27"]
[23,6400300255,"磁性开关","KT-20R","电源DC/AC5-240V;最大电流100mA;功耗10W;两线制","GB/T14048","个",10,"炼钢厂部","2024-07-27"]
[24,6200200977,"单元控制板","TEA4216701000-001","功率单元主控制器;供电电压5-15VDC;功耗100mA;信号输出方式;pwm输出","JB/T8680-2008","块",1,"炼钢厂部","2024-07-27"]
[25,6200200975,"高压变频器功率单元","TEA421760000-001","输入3AC720V;输出AC0-720V/0-50Hz;额定电流330A","JB/T8680-2008","台",2,"炼钢厂部","2024-07-27"]
[26,6200200969,"电源处理板","ERC514-21-23-00","输入AC220V;输出DC300V","JB/T8680-2008","块",1,"炼钢厂部","2024-07-27"]
[27,6200200970,"DDX数字量板","ERC514-10-30-00-01","数字量信号输入、输出采集板24V，24路输入、24路输出","JB/T8680-2008","块",1,"炼钢厂部","2024-07-27"]
[28,6200200972,"DAX模拟入出板","ERC514-10-40-00","低压模拟量信号采集;4-20mA输入、4-20mA输出","JB/T8680-2008","块",1,"炼钢厂部","2024-07-27"]
[29,6200200974,"DAI模拟量板","ERC514-10-10-00","输入输出电流0-5A、输入电压采样0-100V","JB/T8680-2008","块",1,"炼钢厂部","2024-07-27"]
[30,6600300196,"阀门回讯器","TXP-M20GNPM","2xSPDT无源干接点;触点容量10A;250VAC;隔爆型Ex d II C T4;IP67防护等级","GB/T12237","个",6,"炼钢厂部","2024-07-27"]
[31,6100500431,"微型继电器","857-152","线圈电压24VDC;额定电流6A;额定电压250V;辅助触点1OC","GB/T14048","只",10,"炼钢厂部","2024-07-27"]
[32,4100500408,"光电开关","E3Z-LT81-D","连接方式;导线引出（2M）;响应时间1mS;对射型;PNP输出;24VDC","JB/T6475-1992","对",5,"炼钢厂部","2024-07-27"]
[33,4100500409,"APT带灯旋钮开关","PB1S-11CXD/G23","绿色;AC/DC24V;一开一闭;孔径22.5mm;防护等级IP65","IEC60947-5-1","只",10,"炼钢厂部","2024-07-27"]
[34,6400600608,"可调压差开关","DPS100A","Model;A1.0-1/4;触点容量3A;250VAC;IP54防护等级;量程20-200kPa;死区3-70kPa","JB/T8465","只",2,"炼钢厂部","2024-07-27"]
[35,4100400306,"高压绝缘套管","CMZ3-35","电压等级35KV;母排开孔尺寸55mm*125mm;套管内径160mm","JB/DQ2553-1989","只",6,"炼钢厂部","2024-07-27"]
[36,6400600605,"手持式遥控器","CAAJS-2-2","工作电压DC24V;无线遥控有效控制距离不小于100米;镍氢可充电池（两电一充）;遥控发射系统每秒发送8-12个指令数据串;CPU微处理器提供双解码冗余和分集技术;面板采用中文;防护等级IP65","CMMIT ID:2009DJ0390","台",1,"炼钢厂部","2024-07-27"]
[37,6100400406,"接触器","AF1250-30;ABB","Ue=400v Ie=1260A 控制电压100-250V.50-60HZ","IEC60947-2","台",1,"炼钢厂部","2024-07-27"]
[38,6400100050,"取样探头","SAR/TC1200ST","直径35*12 乒乓球型","ISO9001质量标准","支",300,"炼钢厂部","2024-07-27"]
[39,6400400181,"编码器","RCI58B-HS14-2-01024-CA01","\"RADIO-ENERGIE；Ser.Nr.:RE486813460815；Supply:5-30 Vdc\nCHICODE：coder solution...F-91462 MARCOUSS\"","EN 60947-5-2","只",1,"340热轧","2024-07-27"]
[40,6200200986,"变频器风机","BPAB400*4; U1-FAN4-H3","电压等级：48V","GB/T13933","台",1,"能源厂部","2024-07-27"]
[41,6100100251,"故障录波装置","SH-DFR-G","1．采样指标　采样频率 最大 10KHz（9.6KHz）　谐波分辨率 最大 99 次，谐波误差＜ 5%　采样精度 25℃时，额定值下，电流误差＜ 0.2%　25℃时，额定值下，电压误差＜ 0.1%　开关事件分辨率 0.1ms A/D 分辨率 16 位","\"GB/T 22386\t\"","台",1,"能源厂部","2024-07-27"]
[42,6100500432,"电磁吸盘电压检测板","FV1-FV2","输入电压DC170V-260V","IEC97-1991","套",1,"物流中心","2024-07-27"]
[43,6200200925,"风机","HD9FS-FAN-500A-500",23020055,"GB/T14315-2008","台",2,"能源厂部","2024-07-27"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2024年5月电气备件采购项目     项目编号：HG JY-G2024055"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]