{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":60,"n_cols":13,"rows_kept":60,"merged":[[0,0,0,8],[1,0,1,12],[56,0,56,8],[57,0,57,8],[58,0,58,8],[59,0,59,8]],"flags":["formulas_cached_only"]}
["                            （一）开标一览表"]
["项目名称：2022年10月阀门采购项目                     项目编号：HGCGD22130"]
["序号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,7102100008,"法兰式疏水阀","CS49H-25P-40",null,"只",4,null,"烧结","2022-12-27"]
[2,7102000081,"燃气止回阀","HF-G1A","内丝G1\";球头;介质:氧气","只",2,"GB13347-1992","炼钢厂部","2022-12-27"]
[3,7102100008,"法兰式疏水阀","CS49H-25P-40",null,"只",1,null,"高辅工段","2022-12-27"]
[4,5723400001,"不锈钢管端磁化液气动球阀","Q611F-16P DN25","DN25","件",4,"CB/T?4383-2016","管加工厂部","2022-12-27"]
[5,7101900059,"截止阀","HC41X-16C DN80","DN80 原厂家：上海阀门二厂","只",2,"GB/T12233-2006","高辅工段","2022-12-27"]
[6,7101500034,"电动金属硬密封蝶阀","D943P-2.5C","DN400 带输入/输出远程接口 含法兰.垫片","套",10,"GB/T12237","烧结","2022-12-27"]
[7,5500200043,"气动压力调节阀","HTS-16K，DN100","DN100，PN1.6MPa，信号压力：80-240KPa，工作温度-17∽230℃；流量特性:等百分比；阀体材质：WCB,L=348","台",1,"GB/T4213-2008","高炉","2022-12-27"]
[8,7101600185,"电液动调节蝶阀","W1222S-0.6-DN1300","通径DN1300;公称压力0.6MPa；适用温度≤200℃；带液压执行机构及位移传感器，轴承外置，需有加油孔；重量700Kg;不包括液压阀台及电控箱","台",1,"审核图纸","高炉","2022-12-27"]
[9,7101800014,"不锈钢球阀","Q11F-25P-15",null,"只",10,"GB/T 12230-2005","烧结","2022-12-27"]
[10,7101600230,"气动活塞硬密封空气调节阀","法兰式蝶阀通径DN250 阀体、阀板、阀轴材质304不锈钢、双作用气缸、带YT-1000RDM132SOO阀门定位器及过滤器全套;公称压力0.6MPa;","最大流量2500Nm3/h、常用流量1600Nm3/h、最小流量100Nm3/h ;","套",2,"GB/T4213-1992","管加工厂部","2022-12-27"]
[11,7101600231,"气动活塞硬密封空气调节阀","法兰式蝶阀通径DN100 阀体、阀板、阀轴材质304不锈钢、双作用气缸、带YT-1000RDM132SOO阀门定位器及过滤器全套;公称压力0.6MPa;","最大流量100Nm3/h、常用流量450Nm3/h、最小流量40Nm3/h ;","套",2,"GB/T4213-1992","管加工厂部","2022-12-27"]
[12,7101500035,"电动盲板阀","F943X-2.5P","DN400 含防爆电机.控制箱及安装法兰.垫片及紧固件","套",2,"JB/T18527-1997","340热轧","2022-12-12"]
[13,6600300008,"电动蝶阀","D943X-10ZB","工作压力 1.0MPa DN400,配现场操作箱","只",1,"JB/T308-2004","340热轧","2022-12-12"]
[14,6600300009,"电动蝶阀","D943X-10ZB","工作压力 1.0MPa DN350，配现场操作箱","只",1,"JB/T308-2004","340热轧","2022-12-12"]
[15,7102500020,"电动扇形盲板阀","F943X-2.5P；DN350","DN350 ；PN2.5；含防爆电机、防爆控制箱及安装法兰、垫片及紧固件；适用温度：≤250℃；阀体、阀板材质：Q235B；双层波纹管，外316L,内254SMo焊接","套",1,"JB/T18527-1997","340热轧","2022-12-27"]
[16,7102000040,"止回阀","H41H-16-80",null,"只",2,null,"89油管热处理","2022-12-27"]
[17,7100300433,"电磁球阀","AS22061a-G24","常闭，带应急按钮","个",2,"ISO4401","89热轧","2022-12-27"]
[18,7101800154,"高压球阀","KHM-G11/4-1112-01X",null,"件",2,"GB/T9065.2-2010","89油管热处理","2022-12-27"]
[19,7101600047,"手动蝶阀","D341X-80 DN80","压力1.6Mpa DN80","只",8,"GB/T12238-1989","炼钢厂部","2022-12-12"]
[20,7101800120,"三片式不锈钢球阀","Q311F-25P-40","不锈钢手动球阀 浮动直通式 氟塑料 压力2.5mpa DN40","只",80,"GB/T12237","炼钢厂部","2022-12-12"]
[21,7101600186,"气动开关蝶阀","ET101X-1-2-1.6-80-APD80-D","PN1.6Mpa;DN80","只",2,"GB/T12238-2008","炼钢厂部","2022-12-27"]
[22,7101800056,"高压球阀","BKH-25S-1124",null,"只",6,"GB/T9065.2-2010","炼钢厂部","2022-12-12"]
[23,7101800057,"高压球阀","BKH-30S-1125",null,"只",8,"ISO228","炼钢厂部","2022-12-12"]
[24,7101800058,"高压球阀","BKH-38S-1125",null,"只",4,"GB/T9065.2-2010","炼钢厂部","2022-12-12"]
[25,7101800059,"高压球阀","KHB-14SR-1112-03X DIN2353","HYDAC，DIN2353","只",6,null,"炼钢厂部","2022-12-12"]
[26,7101800053,"高压球阀","BKH-16S-1123",null,"只",25,"GB/T12230-2005","管加工厂部","2022-12-12"]
[27,7101800055,"高压球阀","BKH-20S-1123",null,"只",25,"GB/T9065.2-2010","管加工厂部","2022-12-12"]
[28,7101800056,"高压球阀","BKH-25S-1124",null,"只",25,"GB/T9065.2-2010","管加工厂部","2022-12-12"]
[29,7101800057,"高压球阀","BKH-30S-1125",null,"只",25,"ISO228","管加工厂部","2022-12-12"]
[30,7101600125,"手动蝶阀","D341X-16","DN125","只",6,"GB12237-1989","管加工厂部","2022-12-12"]
[31,7101800075,"高压球阀","KHB-M52*2-1212*01X",null,"只",3,"GB/T21465-2008","管加工厂部","2022-12-12"]
[32,7101800155,"高压球阀","KHM-M60*2-1112-01X",null,"件",3,"GB/T9065.2-2010","管加工厂部","2022-12-12"]
[33,7101600114,"气动蝶阀","V637713","1.6MPa;DN250","个",2,null,"管加工厂部","2022-12-12"]
[34,7100100257,"安全阀","A47H-25L-80","压力等级1.6-2.0Mpa；整定压力1.4Mpa","只",1,"GB/T12243-2005","高辅工段","2022-12-27"]
[35,7100100258,"安全阀","A27W-10T-25","压力等级0.8-1.2Mpa；整定压力0.8Mpa","只",2,"GB/T12243-2005","高辅工段","2022-12-27"]
[36,7101600160,"手动蝶阀","D7A1X-10","DN50","只",5,"DL/T746-2001","720厂部","2022-12-12"]
[37,7101900070,"截止阀","J41H-25-250","铸造 GB 8465.3-1987","台",1,"GB 8465.3-1987","高辅工段","2022-12-27"]
[38,7101600232,"电动金属硬密封蝶阀","D943P-2.5C-350","DN350 带输入/输出远程接口 含法兰.垫片；介质：除尘烟气","套",11,"GB/T12237","烧结","2022-12-27"]
[39,7101800054,"高压球阀","BKH-16S-1443",null,"只",10,"GB/T12230-2005","340热轧","2023-01-11"]
[40,7101800055,"高压球阀","BKH-20S-1123",null,"只",10,"GB/T9065.2-2010","340热轧","2023-01-11"]
[41,6600300111,"空气过滤减压阀","YT-200B","出口气压2-8公斤可调","只",5,null,"340热轧","2023-01-26"]
[42,7101800058,"高压球阀","BKH-38S-1125",null,"只",25,"GB/T9065.2-2010","管加工厂部","2023-01-11"]
[43,7101300010,"高压球阀","KHM-50-F6-11141-02X",null,"只",6,null,"管加工厂部","2023-01-11"]
[44,5716000022,"高压泵安全阀","A41Y-320P  DIN24342",null,"只",1,"DIN24342","管加工厂部","2023-02-10"]
[45,7101900062,"截止阀","J41H-16C;","DN125;     1.6MPa;","只",2,"GB/T12237-1989","管加工厂部","2023-01-26"]
[46,7101600052,"手动蝶阀","D343H-2.5","DN300","只",1,"GB/T26144","能源厂部","2023-01-11"]
[47,7101800255,"法兰不锈钢球阀","Q41H-10C-50","1.0MPa;DN50","只",5,"JB/T6376-2005","高炉","2022-12-12"]
[48,7101900055,"不锈钢截止阀","J41W-16P-125",null,"只",1,"GB 8465.3-1987","高炉","2022-12-27"]
[49,7101900022,"不锈钢截止阀","J41W-16P-50","法兰连接直通式不锈钢截止阀 压力1.6MPa DN50","只",1,"GB 8465.3-1987","高炉","2023-01-11"]
[50,7102600017,"气动球阀","Q641PPL-16C-DN50","气动高温球阀 压力1.6mpa DN50 带电磁阀及回迅器","只",3,"GB/T12237","219厂部","2022-12-27"]
[51,7101600162,"气动蝶阀","VF-735DA","DN125","台",2,"GB12224-1989","管加工厂部","2023-01-11"]
[52,7102100003,"法兰式疏水阀","CS49H-16-25","铸造","只",3,null,"烧结","2023-01-11"]
[53,7102100004,"法兰式疏水阀","CS49H-16-32","铸造","只",3,"GB/T12247-1989","烧结","2023-01-11"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2022年10月阀门采购项目           项目编号：HGCGD22130"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":4,"n_cols":1,"rows_kept":4,"merged":[[0,0,0,8],[1,0,1,8],[2,0,2,8],[3,0,3,8]],"flags":["formulas_cached_only"]}
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]