{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、分项报价表","三、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":10,"n_cols":12,"rows_kept":10,"merged":[[0,0,0,7],[1,0,1,11],[6,0,6,7],[7,0,7,7],[8,0,8,7],[9,0,9,7]],"flags":["formulas_cached_only"]}
["                            （一）开标一览表"]
["项目名称：2023年11月炼铁技改洗车机采购项目                     项目编号：HGJS-G2023056"]
["序号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,"全自动智能洗车机","全自动龙门洗车机：封闭框架20×5.5×5.5m；洗车速度：12～60；清洗车辆限制：长18×宽3.3×高4.5m；通过车辆最大重量：150；清洗时间：60～300s/辆；清洗方式：清洗段10m，2台水泵冲洗+颠簸抖尘风干段10m，4台风机吹干+颠簸抖水；清洗部位：轮胎、车身；启动方式：自动/手动/人机界面；装机总功率≈115kw:2×30冲洗+22冲淤+7.5清淤+4×5.5风机+2照明道闸等，清淤泵不同时工作；水源供给：冲洗水回水池沉淀过滤后循环利用DN50阀门自动补水；适应工作环境相对湿度：≤90%；安全过载率130；控制系统：西门子PLC，触摸屏等电器；","洗车机洗完后无污染，要有记录包括影视","套",1,"详见技术规格书","炼铁原料场封闭项目（HG202317）","2023-11-20"]
[]
[]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、分项报价表","index":2,"n_rows":19,"n_cols":7,"rows_kept":19,"merged":[[0,0,0,6],[1,0,1,6],[12,1,12,3],[13,0,13,6],[15,0,15,6],[16,0,16,6],[17,0,17,6],[18,0,18,6]],"flags":["formulas_cached_only"]}
["（二）分项报价表"]
["项目名称：2023年11月炼铁技改洗车机采购项目                     项目编号：HGJS-G2023056"]
["序号","物资名称","单位","数量","单价\n（万元）","合价\n（万元）","备注"]
[1]
[2]
[3]
[4]
[5]
[6]
[7]
[8]
[null,"…"]
[null,"小计"]
["总价（大写）"]
[]
["注：如免去某些费用，请在报价栏内注明“免费”字样（所有报价均为含税价）"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"三、商务 技术偏离表","index":3,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （三）商务/技术偏离表"]
["项目名称：2023年11月炼铁技改洗车机采购项目                     \n项目编号：HGJS-G2023056"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]